Justin Shapiro

20140528

CDOM REF Prep

Reference Fluid

1. Eco 20 Carboy
2. Acid Washed Glass 2x Beaker
3. Acid Wash Filter 2x, 15 minute dwell
4. RO Rinse syringe 2x
5. RO Rinse filter 4x
6. Eco20 Rinse Filter – Discard Filtrate
7. Filter desired volume of Eco20
8. IF HIGH PRESSURE, PLACE UNDER VACUUM FOR 2.5 HR+

Reference Bag

1. Acid Soak at least 1hr, up to 2 days
2. Acid Rinse
3. RO Rinsex3
4. ECO20 Rinse
5. Fill Bag

Take sample for Camia to run on bench spec.